**Assignment -3**

Python Programming

|  |  |
| --- | --- |
| Assignment Date | 29 September 2022 |
| Student Name | Mr. Biplab Das S |
| Student Roll Number | 714019106015 |
| Maximum Marks | 2 Marks |

**Question-1:**

Write a python code for blinking LED and Traffic Lights for Raspberry Pi. Only python code is enough, no need to execute in Raspberry Pi. Note you are allowed to use web search and complete the assignment.

#Python code for blinding LED

import RPi.GPIO as GPIO # Import Raspberry Pi GPIO library

from time import sleep # Import the sleep function from the time module

GPIO.setwarnings(False) # Ignore warning for now

GPIO.setmode(GPIO.BOARD) # Use physical pin numbering

GPIO.setup(8, GPIO.OUT, initial=GPIO.LOW) # Set pin 8 to be an output pin and set initial value to low (off)

while True: # Run forever

GPIO.output(8, GPIO.HIGH) # Turn on

sleep(1) # Sleep for 1 second

GPIO.output(8, GPIO.LOW) # Turn off

sleep(1) # Sleep for 1 second

#Traffic lights for Raspberry Pi  
import RPi.GPIO as GPIO

import time

import signal

import sys

# Setup

GPIO.setmode(GPIO.BCM)

GPIO.setup(9, GPIO.OUT)

GPIO.setup(10, GPIO.OUT)

GPIO.setup(11, GPIO.OUT)

# Turn off all lights when user ends demo

def allLightsOff(signal, frame):

GPIO.output(9, False)

GPIO.output(10, False)

GPIO.output(11, False)

GPIO.cleanup()

sys.exit(0)

signal.signal(signal.SIGINT, allLightsOff)

# Loop forever

while True:

# Red

GPIO.output(9, True)

time.sleep(3)

# Red and amber

GPIO.output(10, True)

time.sleep(1)

# Green

GPIO.output(9, False)

GPIO.output(10, False)

GPIO.output(11, True)

time.sleep(5)

# Amber

GPIO.output(11, False)

GPIO.output(10, True)

time.sleep(2)

# Amber off (red comes on at top of loop)

GPIO.output(10, False)

